Airport Information

Departure

Airport | ICAO | Alt | ATIS | Ground | Tower | Clearance
Hannover | EDDV | 183 | 132.12 | 121.95 | 120.22 120.17 |

Rwy-ID | Hdg | Len (ft) | Surface | ILS | DME | Closed
09L | 0.1 | 12443 | Concrete | 108.30 | 113.95
09R | 0.1 | 7659 | Concrete | 108.70 | 116.90 | Closed
09C | 0.1 | 2231 | Asphalt |  |
27L | 0.3 | 7659 | Concrete | 109.50 | 116.90 | Closed
27R | 0.3 | 12443 | Concrete | 108.90 | 113.95
27C | 0.3 | 2231 | Asphalt |  |

Rwy 27R South "ELNAT 7S" with NIE (116.50)
Inbound HW; at 3.5 DME HAD LT, on track 212° HW to
intercept R173 NIE; on R173 NIE via MEGEL to TOLTA;
on track 165° to ELNAT.
Climb with 7% (425ft/NM) until passing 3500.

Arrival

Airport | ICAO | Alt | ATIS | Ground | Tower | Approach
Nurnberg | EDDN | 1046 | 123.07 | 118.10 | 118.30 | 118.97 119.52 119.47

Rwy-ID | Hdg | Len | Surface | ILS | DME
10 | 0.1 | 8841 | Concrete | 111.30 |
28 | 0.3 | 8841 | Concrete | 109.10 |